1.Step 1: Prepare to upgrade the environment

Configure computer IP: 192.168.1.104

Preparing to upgrade the catalog: including cfe, olt program, web program

Open the tftp tool and select the upgrade directory

2.Step 2: Enter boot view, upgrade boot, and restart

CFE> ifconfig eth0 -addr=192.168.1.100 -mask=255.255.255.0

CFE> flash -noheader 192.168.1.104:FD1108S\_CFE\_200731.bin flash0.boot

CFE> reset -cpu

3.Step 3: Enter the boot view and erase the partition

CFE> erase flash flash0.os

CFE> erase flash flash0.os2

CFE> erase flash flash0.fs

4.Step 4: Enter the boot view, upgrade the program, and restart

CFE> ifconfig eth0 -addr=192.168.1.100 -mask=255.255.255.0

CFE> flash -noheader 192.168.1.104:FD11xxS\_V2.4.xx\_180517\_X000.img flash0.os

CFE> flash -noheader 192.168.1.104:FD11xxS\_FW2.4.xx\_180517\_X000.img flash0.os2

CFE> reset -cpu

5.Step 5: Enter the command line view and upgrade the Web program

Username:admin

Password:

epon# system update web-server FD11xxS\_WEB\_V1.2.xx\_X000\_180517\_1326.img tftp-server 192.168.1.104